When using related industrial protocol files, make sure that the firmware version and protocol configuration file of devices meet the following requirements:

| Model                             | Firmware Version   | EthernetIP Configuration File      | PROFINET Configuration File                    |
|--------------------------------------|---------------------|-----------------------------------|-------------------------------------------------|
| ID800 series (including IDA**X)      | V3.0.0 and later   | smart_camera_id800.eds           | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| ID2000 series (including IDB**X)     | V3.0.0 and later   | smart_camera_id2000.eds          | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| ID3000 series (including IDC**X)     | V2.4.0 and later   | smart_camera_id3000.eds          | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| ID3000X series (including IDCX**X)   | V3.0.0 and later   | smart_camera_id3000.eds          | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| ID5000 series (including IDE**X)     | V2.4.0 and later   | smart_camera_id5000.eds          | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| ID5000X series                       | V3.2.2 and later   | smart_camera_id5000.eds          | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| IDH5000 series                       | V1.0.4 and later   | smart_camera_idh5000.eds         | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| IDH7000P series                      | V1.0.4 and later   | smart_camera_idh.eds             | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| IDH7000B series                      | V1.0.0 and later   | smart_camera_idh.eds             | GSDML-V2.34-Hikvision-MV-20220314.xml         |
| SC2000A series navigation sensor     | V2.8.0 and later   | smart_camera_sc2000a.eds         | GSDML-V2.34-Hikvision-MV-20220314.xml         |


Note:
-Configuration files can be obtained from the same folder as this document.
-For IDH7000 with firmware version V2.0.0 or V2.0.1, the configuration file is smart_camera_idh5000.eds; For IDH7000 with firmware version V2.0.2 and later, the configuration file is smart_camera_idh.eds.



