When using industrial protocols, the minimum firmware version requirements for each device series and their corresponding Ethernet/IP and PROFINET configuration files are as follows:

| Model                                 | Firmware Version    | EthernetIP Configuration File| PROFINET Configuration File                |
|---------------------------------------|---------------------|------------------------------|--------------------------------------------|
| SC1000 Series Vision Sensor           | V1.0.0 and later    | smart_camera_sc1000.eds      | GSDML-V2.34-Hikvision-MV-20250409.xml      |
| SC2000E Series Vision Sensor          | V2.0.0 and later    | smart_camera_sc2000e.eds     | GSDML-V2.34-Hikvision-MV-20250409.xml      |
| SC2000X Series Vision Sensor          | V2.0.0 and later    | smart_camera_sc2000x.eds     | GSDML-V2.34-Hikvision-MV-20250409.xml      |
| SC2000E (Mini) Series Vision Sensor   | V2.0.0 and later    | smart_camera_sc2000e.eds     | GSDML-V2.34-Hikvision-MV-20250409.xml      |
| SC3000 Series Vision Sensor           | V2.0.0 and later    | smart_camera_sc3000.eds      | GSDML-V2.34-Hikvision-MV-20250409.xml      |
| SC3000X Series Vision Sensor          | V3.1.0 and later    | smart_camera_sc3000.eds      | GSDML-V2.34-Hikvision-MV-20250409.xml      |
| SC5000X Series Smart Camera           | V4.2.30 and later   | vm4xx.eds                    | GSDML-V2.34-Hikvision-VM4XX-20250908.xml   |
| SC6000 Series Smart Camera            | V4.2.30 and later   | vm4xx.eds                    | GSDML-V2.34-Hikvision-VM4XX-20250908.xml   |

Note:
-Configuration files can be obtained from the same folder as this document.