Recommended Firmware and Client Version Compatibility Information:
+--------------+----------------------+-----------------+
| Device Series  | Firmware Version    |Client Version    |
+--------------+----------------------+-----------------+
| SC2000x Series |  V4.3.6             | V3.2.3           |
+--------------+----------------------+-----------------+
******************************************************
Update Date：2026-07-01
Version Number：4.3.6
******************************************************
1.Added light source selection, and fixed known issues with light source selection.
2.The maximum number of schemes that can be created has been changed to 32.  
3.Due to the eMMC switching in the SC2000x series, version isolation has been added during firmware upgrades.

******************************************************
Update Date：2026-04-14
Version Number：4.3.4   
******************************************************
1. Added SC2013XC, SC2013XM, SC2020XM, SC2020XC models.
2. Added wide dynamic range parameters for SC2013X, SC2020X, and SC2023X camera models. Added digital wide dynamic range parameters for SC2020X.
3. Added presence detection, learning-based counting, and multi-target counting.
4. Presence detection, learning-based counting, and multi-target counting support circular output function.
5. For SC2020X model IO output, removed the exposure output type.
6. Added security field "SE V4.1" in device version.
7. Optimized template contour point display for reference image, pattern counting, pattern presence, contour presence, and contour counting.
8. Optimized interface display of color measurement module.
9. Code recognition added configuration parameter: Code39 FULL ASCII enable configuration.
10. Fixed the issue where parameters become inconsistent after camera restart when modifying configuration parameters in the IO allocation interface.

